(footprint "IND_HPC6045NC_TTA"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(tags "HPC6045NC-1R5M ")
	(property "Reference" "L1"
		(at 0 4.25 180)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "d4bae5be-9186-4bd9-b590-a86048d460f0")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Value" "1.5uH"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "8b39c0c6-720a-4dd1-add8-ef370345f4f5")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "117fdfc5-dd3e-4e23-8f2b-b00bedf16ba2")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Inductor with iron core"
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
		(uuid "d2b93cd5-64c1-4021-8d2f-d88cfc9716d1")
		(effects
			(font
				(size 1.27 1.27)
				(thickness 0.15)
			)
		)
	)
	(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
	(sheetname "/EPS/")
	(sheetfile "eps.kicad_sch")
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_line
		(start -0.40365 3.2766)
		(end 0.40365 3.2766)
		(stroke
			(width 0.1524)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "6281deb6-c9f3-4a67-8987-2a1363bc26f6")
	)
	(fp_line
		(start 0.40365 -3.2766)
		(end -0.40365 -3.2766)
		(stroke
			(width 0.1524)
			(type solid)
		)
		(layer "F.SilkS")
		(uuid "daa09bef-bae9-4597-bcc9-992eb875ed96")
	)
	(fp_circle
		(center -4.4196 0)
		(end -4.3434 0)
		(stroke
			(width 0.1524)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "6237cd69-bad6-46d2-93af-c9540e9be314")
	)
	(fp_rect
		(start -3.578645 -3.450093)
		(end 3.549318 3.405577)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "bf7ac776-e830-4d2e-afce-87c5e5545369")
	)
	(fp_line
		(start -3.1496 -3.1496)
		(end -3.1496 3.1496)
		(stroke
			(width 0.0254)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "718983f3-1d74-416f-9e79-42e45b6bb66d")
	)
	(fp_line
		(start -3.1496 3.1496)
		(end 3.1496 3.1496)
		(stroke
			(width 0.0254)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "160deba8-7a56-4edb-b305-e16cae23fbaa")
	)
	(fp_line
		(start 3.1496 -3.1496)
		(end -3.1496 -3.1496)
		(stroke
			(width 0.0254)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "a2267678-c6a3-43ae-ae5c-3a5fb574c376")
	)
	(fp_line
		(start 3.1496 3.1496)
		(end 3.1496 -3.1496)
		(stroke
			(width 0.0254)
			(type solid)
		)
		(layer "F.Fab")
		(uuid "24537910-9417-42a0-8486-c0d6df9c2e32")
	)
	(fp_circle
		(center -2.6416 0)
		(end -2.5654 0)
		(stroke
			(width 0.0254)
			(type solid)
		)
		(fill no)
		(layer "F.Fab")
		(uuid "1c6bcb2c-a75a-4b30-8afa-7d58c75a5271")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "311e0f22-3eff-4c4c-bfb9-a5681753b07c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at -2.0066 0 90)
		(size 6.2992 2.5908)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "350e22b6-ef7b-453d-a24e-c37f64479f4f")
	)
	(pad "2" smd rect
		(at 2.0066 0 90)
		(size 6.2992 2.5908)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "0b9f03a3-58ed-4bf2-bfbd-4eb175b73555")
	)
	(zone
		(layer "F.Cu")
		(uuid "a4beb9f8-4a55-4db3-8f45-d96fed7d0f9c")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy -3.0988 -3.0988) (xy 3.0988 -3.0988) (xy 3.0988 -3.2004) (xy -3.0988 -3.2004)
			)
		)
	)
	(zone
		(layer "F.Cu")
		(uuid "54ab095d-8140-45c2-8445-da7861039611")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy -3.0988 3.2004) (xy 3.0988 3.2004) (xy 3.0988 3.0988) (xy -3.0988 3.0988)
			)
		)
	)
	(zone
		(layer "F.Cu")
		(uuid "9c3d0018-2ac1-46bb-b256-30f8f82114bd")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy -0.6604 -3.2004) (xy 0.6604 -3.2004) (xy 0.6604 3.2004) (xy -0.6604 3.2004)
			)
		)
	)
	(embedded_fonts no)
	(model "${KIPRJMOD}/3dmodels/IND_HPC6045NV_TTA.iges"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
